================================================================================
  NX7700x/A2010L-60,A2010M-60,A2010M-30,A2010M-15 LAN Driver Module(V17.2)
                                    (Windows Server 2012 R2/Windows Server 2012)
================================================================================
                                                                NEC Corporation
                                                                     July 2016
[Table of contents]
1.About the software
2.Models
3.Driver install procedures  
4.Notes
5.Update history
6.Trademarks and copyright
--------------------------------------------------------------------------------

1.About the software
  "NX7700x/A2010L-60,A2010M-60,A2010M-30,A2010M-15 LAN Driver Module(V17.2)" 
  ("the Software"), for Windows Server 2012 R2, Windows Server 2012, will make 
  the enhancements or solve the issues for NEC NX7700x series products as below.

2.Models
   NX7700x/A2010L-60,A2010M-60,A2010M-30,A2010M-15

3.Driver install procedures

 Perform the following steps to extract the Software and install the driver.
 - How to extract:
 (1) Download GVO-009853-G01_xxxxxxxxxxxxxxxxxx.zip(x is an expression of arbitrary 
     numbers) to any directory. (for example, "C:\TEMP" folder) 
 (2) Extract GVO-009853-G01_xxxxxxxxxxxxxxxxxx.zip(x is an expression of arbitrary 
     numbers).
     Note: You must not use the folder with the name including space (" ")
           in extracting the zip file.
 
 - How to install:
 (1) Install the driver by referring to "LAN Driver Installation Guide 
    (Broadcom v17.2)" (v172_InstallationGuideNX7700x.pdf).

4.Notes
  Refer to [v172_InstallationGuideNX7700x.pdf] for installation notes.

5.Update history
  July 2016
  <Bug fix>
  The following problems are fixed in the Software.
   1) In the environment of using Broadcom NetXtreme 1-gigabit network adapters,
      the following problems occur, when VMQ is Enabled.
      -Virtual machine on Hyper-v cannot connect to network.
      -vNIC on Host OS of Hyper-v cannot connect to network.

   2) In the environment of using Broadcom NetXtreme 1-gigabit network adapters
      (BCM 5719), the following problems occur when you power on the server 
      from AC OFF state.
      -Virtual machine on Hyper-v cannot connect to network.
      -Virtual machine on Hyper-v cannot be shut down.
      -It cannot connect to network by LAN port.
      -Windows cannot be booted normally.

6.Trademarks and copyright
  *Microsoft, Windows, Windows Server are registered trademarks or trademarks of
   Microsoft Corporation in the United States and other countries.
  *Broadcom, the pulse logo, Connecting everything, the Connecting everything
   logo, NetXtreme, Ethernet@Wirespeed, LiveLink, and Smart Load Balancing
   are among the trademarks of Broadcom Corporation and/or its affiliates in 
   the  United States, certain other countries, and/or the EU.
  *All other product, brand, or trade names used in this publication are the 
   trademarks or registered trademarks of their respective trademark owners.
