===========================================================================
 Universal RAID Utility Ver5.0 (Linux Edition)
 for NEC NX7700x Series
===========================================================================
                                                            NEC Corporation
                                                                   Mar 2020

[Contents]
  1. Software Introduction
  2. Applicable model
  3. Installation Procedure
  4. General Notice
  5. Revision History
---------------------------------------------------------------------------

1. Software Introduction
Universal RAID Utility (hereinafter called "this software") is RAID System
Management Utility for the following applicable models.

2. Applicable model
  <NX7700x server>
  - NX7700x/A4012M-4
  - NX7700x/A4012L-2
  - NX7700x/A4012L-1
  - NX7700x/A4010M-4
  - NX7700x/A5012M-4
  - NX7700x/A5012L-2
  - NX7700x/A5010M-4
  - NX7700x/A5012L-2D
  - NX7700x/A5012L-1D
  - NX7700x/A5010M-4 v2
  - NX7700x/A5012M-4 v2
  - NX7700x/A5012L-2 v2
  - NX7700x/A5012L-2D v2
  - NX7700x/A5012L-1D v2
  <RAID Controllers>
  - NE3303-177 RAID Controller (1GB, RAID 0/1/5/6)
  - NE3303-178 RAID Controller (2GB, RAID 0/1/5/6)
  - NE3303-H004 RAID Controller (2GB, RAID 0/1/5/6)
  - NE3303-207 RAID Controller (2GB, RAID 0/1/5/6)
  - NE3303-207L RAIDコントローラ (2GB, RAID 0/1/5/6)
  - NE3303-208 RAID Controller (4GB, RAID 0/1/5/6)
  - NE3303-208L RAIDコントローラ (4GB, RAID 0/1/5/6)
  For users who will install following Linux on NEC NX7700x series.
  - Red Hat Enterprise Linux 7.6
  - Red Hat Enterprise Linux 7.7

3. Installation Procedure
  Refer to the "Universal RAID Utility User's Guide" which is contained
in the installation image for the detailed procedure of the installation.

4. General Notice
  (1) Restart of the server after Universal RAID Utility installation
      /update/uninstallation by ExpressUpdate.
      When you install, update, or uninstall Universal RAID Utility with
      the Automatic Reboot checkbox checked, "Installation Failed" or
      "Reboot Required" may be displayed as the current status. 
      In this case, the installation, update, or uninstallation has
      been successfully finished. However, you must restart the server
      where you install Universal RAID Utility. If you leave the server
      without restart, Universal RAID Utility will not operate properly.

5. Revision History
  2020/3/6    Ver5.0 Rev 3589
  "Enhancement"
     1.  Additional support of the following OS
        - Red Hat Enterprise Linux 7.7
     2.  Additional support of the applicable model
        - NX7700x/A5012L-2D v2
        - NX7700x/A5012L-1D v2
     3.  Additional support of the following RAID Controllers
        - NE3303-207L RAID Controller (2GB, RAID 0/1/5/6)
        - NE3303-208L RAID Controller (4GB, RAID 0/1/5/6)

  2019/10/31  Ver5.0 Rev 3589
  "Enhancement"
     1.  Additional support of the applicable model
        - NX7700x/A5010M-4 v2
        - NX7700x/A5012M-4 v2
        - NX7700x/A5012L-2 v2
     2.  Additional support of the following RAID Controllers
        - NE3303-207 RAID Controller (2GB, RAID 0/1/5/6)
        - NE3303-208 RAID Controller (4GB, RAID 0/1/5/6)

  2019/7/16  Ver5.0 Rev 3589
  "Enhancement"
     1.  Additional support of the applicable model
        - NX7700x/A4012M-4
        - NX7700x/A4012L-2
        - NX7700x/A4012L-1
        - NX7700x/A4010M-4

  2019/6/5  Ver5.0 Rev 3589
  First version released.
  "Enhancement"
     1.  Additional support of the following OS
        - Red Hat Enterprise Linux 7.6

