Intel® Chipset Device Software

10.1.2.80

Release Notes

August 23, 2016

Microsoft Windows* 7

Microsoft Windows* 7 x64

Microsoft Windows* Server 2008 R2 x64

Microsoft Windows* 8

Microsoft Windows* 8 x64

Microsoft Windows* Server 2012 x64

Microsoft Windows* 8.1

Microsoft Windows* 8.1 x64

Microsoft Windows* Server 2012 R2 x64

Microsoft Windows* 10 (only for Intel® Atom™ / Celeron®/ Pentium® Processor)

Microsoft Windows* 10 x64

Microsoft Windows* Server 2016 x64

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH INTEL PRODUCTS. NO LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO ANY INTELLECTUAL PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT. EXCEPT AS PROVIDED IN INTEL’S TERMS AND CONDITIONS OF SALE FOR SUCH PRODUCTS, INTEL ASSUMES NO LIABILITY WHATSOEVER AND INTEL DISCLAIMS ANY EXPRESS OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF INTEL PRODUCTS INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A PARTICULAR PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY PATENT, COPYRIGHT OR OTHER INTELLECTUAL PROPERTY RIGHT.

A “Mission Critical Application” is any application in which failure of the Intel Product could result, directly or indirectly, in personal injury or death. SHOULD YOU PURCHASE OR USE INTEL’S PRODUCTS FOR ANY SUCH MISSION CRITICAL APPLICATION, YOU SHALL INDEMNIFY AND HOLD INTEL AND ITS SUBSIDIARIES, SUBCONTRACTORS AND AFFILIATES, AND THE DIRECTORS, OFFICERS, AND EMPLOYEES OF EACH, HARMLESS AGAINST ALL CLAIMS COSTS, DAMAGES, AND EXPENSES AND REASONABLE ATTORNEYS’ FEES ARISING OUT OF, DIRECTLY OR INDIRECTLY, ANY CLAIM OF PRODUCT LIABILITY, PERSONAL INJURY, OR DEATH ARISING IN ANY WAY OUT OF SUCH MISSION CRITICAL APPLICATION, WHETHER OR NOT INTEL OR ITS SUBCONTRACTOR WAS NEGLIGENT IN THE DESIGN, MANUFACTURE, OR WARNING OF THE INTEL PRODUCT OR ANY OF ITS PARTS.

Intel may make changes to specifications and product descriptions at any time, without notice. Designers must not rely on the absence or characteristics of any features or instructions marked “reserved” or “undefined”. Intel reserves these for future definition and shall have no responsibility whatsoever for conflicts or incompatibilities arising from future changes to them. The information here is subject to change without notice. Do not finalize a design with this information.

The products described in this document may contain design defects or errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.

Contact your local Intel sales office or your distributor to obtain the latest specifications and before placing your product order.

Code names featured are used internally within Intel to identify products that are in development and not yet publicly announced for release. Customers, licensees and other third parties are not authorized by Intel to use code names in advertising, promotion

The Intel® Chipset Device Software may contain design defects or errors described as “known issues” which may cause the product to deviate from expected performance. Current characterized known issues are documented in this update.

Intel and the Intel logo are trademarks of Intel Corporation in the U.S. and other countries.

*Other names and brands may be claimed as the property of others.

Copyright © 2015, Intel Corporation. All rights reserved.

Revision History

Date | Driver Revision | Description | Build Number
June 12, 2015 | 10.1.2.6 | PC | 6
July 8, 2015 | 10.1.2.8 | PV | 8
July 31, 2015 | 10.1.2.9 | PV | 9
August 12, 2015 | 10.1.2.10 | PV | 10
January 22, 2016 | 10.1.2.19 | PV | 19
May 22, 2016 | 10.1.2.70 | PV | 70
June 17, 2016 | 10.1.2.73 | PV | 73
July 7, 2016 | 10.1.2.74 | PV | 74
August 3, 2016 | 10.1.2.77 | PV | 77
August 23, 2016 | 10.1.2.80 | PV | 80

Intel® Chipset Device Software Support

The Intel® Chipset Device Software contains support for the following:

§ Intel® Xeon Phi® Processor x200 product family

§ Intel® Xeon® Processor E7-4800/8800 v4 product family

§ Intel® Xeon® Processor E7-4800/8800 v3 product family

§ Intel® Xeon® Processor E7-4800/8800 v2 product family

§ Intel® Xeon® Processor E7-2600 v4 product family

§ Intel® Xeon® Processor E5-2600 v4 product family

§ Intel® Xeon® Processor E5-2600 v3 product family

§ Intel® Xeon® Processor E5-2600 v2 product family

§ Intel® Xeon® processor E3-1500 v5 product family

§ Intel® Xeon® processor E3-1200 v6 product family

§ Intel® Xeon® processor E3-1200 v5 product family

§ Intel® Xeon® processor E3-1200 v4 product family

§ Intel® Xeon® processor E3-1200 v3 product family

§ Intel® Xeon® processor E3-1200 v2 product family

§ Intel® Xeon® Processor D-1500 product family

§ 3rd Gen Intel® Core® i7 processor product family

§ 4th Gen Intel® Core® i7 processor product family

§ 5th Gen Intel® Core® i7 processor product family

§ 6th Gen Intel® Core® i7 processor product family

§ Intel® Atom™ Processor S1200 product family

§ Intel® Atom™ Processor C3000 product family

§ Intel® Atom™ Processor C2000 product family

§ Intel® C610 series chipset

§ Intel® C600 series chipset

§ Intel® C230 series chipset family

§ Intel® C220 series chipset family

§ Intel® C210 series chipset family

§ Intel® C200 series chipset family

§ Intel® 100 series chipset family

§ Intel® X99 chipset family

§ Intel® X79 series chipset family

§ Intel® 8 series chipset family

§ Intel® 7 series chipset family

§ Intel® 6 series chipset family

§ Intel® Communications Chipset 8900 Series

New Features

Features Added in Build 10.1.2.80
ID | Description
1 | Purley - Removed support for USB3 controller
2 | Fixed issue with 2016 certification. Previous build was failing 2016 Signed driver test
Features Added in Build 10.1.2.77
ID | Description
1 | RS1/Server 2016 RTM certified
2 | Branding string for KBL updated
3 | 5918 DRAM device added for KBL
4 | removed ISH devices from this PCHs: ICL, CNL, KBL, SPT
5 | NULL HECI version/date fixed
Features Added in Build 10.1.2.74
ID | Description
1 | PC level and fully certified for Denverton
Features Added in Build 10.1.2.70
ID | Description
1 | Intel® Xeon® Processor E7-2600 v4 product family added "Core i7" to end of branding string
Features Added in Build 10.1.2.19
ID | Description
1 | Added device IDs for higher core count Intel® Xeon® Processor E7-2600 v4 product family procs.
Features Added in Build 10.1.2.10
ID | Description
1 | Fix issues on USB controller devices 8D2D and 8D26 for Intel® C610 series/X99 chipset.
Features Added in Build 10.1.2.9
ID | Description
1 | Fixed a few yellow bangs on Intel® Xeon® Processor E5-2600 v4 product family
2 | Intel® Xeon® processor E3-1200 v5 product family final updates
Features Added in Build 10.1.2.8
ID | Description
1 | Broadwell-DE (Intel(R) Xeon(R) E7 v4 / Xeon(R) E5 v4 / Xeon(R) E3 v4 / Xeon(R) D) few devices branding update
2 | NULL HECI going public
3 | Few KnightsLanding devices added for YBR
Features Added in Build 10.1.2.6
ID | Description
1 | Intel® Xeon® processor E3-1200 v5 product family branding update
2 | Intel® Xeon® Processor E5-2600 v3 product family branding update
3 | Intel® Xeon® Processor D-1500 product family branding update
4 | NULL HECI integration for Greenlow, Patsburg, Wellburg
5 | Lewisburg device update

Issues Resolved

Issues Resolved in Build 10.1.2.6
ID | Description
1 | Installer didn’t prompt user to reboot when reboot was required.

Known Issues

Known Issues in Build 10.1.2.8
ID | Description
1 | The 1911 GGM device will show yellow bang after the installation. This GGM device is not for server platform usage. Please disable GMM in SBIOS to avoid unnecessary issues.